[bookmark: _Toc6586]Wi-Fi Configuration Activation Process
The activation process for connecting to the network over Wi-Fi when the user is not using a wired (Ethernet) connection.
Step 1: Make sure Bluetooth is turned on for your phone. You can then access the device list, find your device name (for first-time activation, the device name is the SN number on the bottom of the device — locate the matching SN number), and tap Activate;
[image: 36b25739989e46d7987f1dafb87215f7]
Step 2: A “Network not connected” page pops up during activation; tap Go to Configure.
[image: c145d49c44062cf378c76a4560fbf55e]
Step 3: Find the corresponding Wi-Fi network, enter the correct Wi-Fi password, and tap Connect to Wi-Fi.

[image: 08a4dec20404197eb17cce747eef21b1][image: e172db7bd43d57be6b056e5edf4e95d9]

Step 3: Once connected, proceed to storage mode initialization — the RAID mode can be selected as needed (RAID 0 by default; see Table 1 for details on each RAID mode).
[bookmark: _GoBack][image: e172db7bd43d57be6b056e5edf4e95d9][image: 6122cba7e92f65e0a2a74049c7132b2e]
Step 4: Tap Initialize. A confirmation button pops up on the page; tap Confirm to enter the device management home page, and the device is ready for normal use.
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